**SCOPE OF WORK FOR SUPPLY DRINKING WATER TANKER**

1. The chassis will be supplied by the manufacturer.
2. A 6x4, full forward control, any suitable indigenous make, BHARAT STAGE IV EURO IV) chassis engine along with single cabin and P.T.O. with factory built cabin for 6 personnel including driver.
3. Fabrication and mounting of 12 KL capacity water tank as per standard specification.
4. Supply and mounting of high & low pressure firefighting pump as per specification.
5. Supply and mounting of water monitor.

**USE**

The Water Tanker shall be used to carry the water for firefighting / drinking water tank refilling purposes. The pump will be driven by P.T.O.

The below mentioned terms and conditions are applicable for the vehicle.

1. Effective date of hiring 1st July 2023 truck mounted water tanker capacity of 12 KL and it should be commercial passing, including driver, maintenance, fuel, consumable etc.
2. Required to provide one driver for 12 hours. Hiring and two drivers for 24 hours and also hiring two helpers for 24 hours (Day & Night), Lodging and boarding expenses of drivers and helpers are to be borne by service provider
3. In case vehicle shall be break down and alternative vehicle must be arranged by service provider.
4. The cost of fuel, Oil and maintenance will be borne by service provider.
5. Contractor should submit all the relevant documents to Administration Department time to time.  The documents are driving licence, Registration Certificate, Road Tax, Permit, fitness certificate, Population under control certificate, Insurance copy and Addhar Card of driver and Helpers.  If valid documents could not provide on time, work order get cancelled immediately.
6. Contractor shall maintain a record for refilling of water tank inside and outside the port operational.
7. In case of accident of vehicle, it will be the responsibility to service provider to launch complaint and repair of water tanker including settlement of insurance claim.
8. The bill in the prescribed format should be submitted by 1st of every month along with duly certified water supply record / details.  The invoice should be raised as per GST regime.
9. If company found any civil and criminal offences involved by you and your driver / Helpers jointly or separately effecting directly to company, then the work order will be terminated immediately.

Commercial

|  |  |  |
| --- | --- | --- |
| **Description** | **Unit** | **Rate** |
| Hiring of Truck mounted drinking water tanker 12 KL capacity to supply fresh water to entire port area in tanks, Sumps, Tugs etc, with1. Drivers helpers on shift wise (driver should have taxi passing license)
2. Safety belt in all seats
3. Tracking system (GPRS)
4. Reverse horn
5. Speed Governor
6. Seating capacity – two person
7. Taxi passing
8. Power steering
9. Valid owner ship
10. Full insurance
11. Drivers and attendant should have with uniform Safety shoes and florescent jacket compulsory
12. Hose pipe to be provided by contractor – 25 ft
 | Month | Rs. /- per month |
| Availability of truck mounted tanker with driver and helper |  | 24 hour basis |
| Diesel, lube oil and other required consumables |  | On contractor a/c |